Switch#sh run

Building configuration...

Current configuration : 4441 bytes

!

! No configuration change since last restart

! NVRAM config last updated at 13:11:02 UTC Fri Feb 18 2000

!

version 15.0

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname Switch

!

boot-start-marker

boot-end-marker

!

!

no aaa new-model

switch 1 provision ws-c2960x-24td-l

!

!

!

!

crypto pki trustpoint TP-self-signed-2470993664

enrollment selfsigned

subject-name cn=IOS-Self-Signed-Certificate-2470993664

revocation-check none

rsakeypair TP-self-signed-2470993664

!

!

crypto pki certificate chain TP-self-signed-2470993664

certificate self-signed 01

3082022B 30820194 A0030201 02020101 300D0609 2A864886 F70D0101 05050030

31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274

69666963 6174652D 32343730 39393336 3634301E 170D3030 30323138 31333131

30315A17 0D323030 31303130 30303030 305A3031 312F302D 06035504 03132649

4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 34373039

39333636 3430819F 300D0609 2A864886 F70D0101 01050003 818D0030 81890281

8100A3CC 16B9AAB7 464D73E2 694ED057 4627A881 F6EF39FB 4E77C77B 9308D2E0

AC148897 D63F56D6 23E52258 1106968E CE1499BC E151115A F073C4F1 F95860FA

27A3BB9B 2C2478CF 8A6AEB81 38114734 6F5DFB41 D45041AE 1226BD64 5804E066

CFCFB660 8C5DECE8 F1B792D9 1C5791AC D00A9F7A 4F5D5354 1D7A9C3C 57E71FDD

95410203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 301F0603

551D2304 18301680 1415F107 8881A98C 9B534CFD 04059F98 58D7E2CF EE301D06

03551D0E 04160414 15F10788 81A98C9B 534CFD04 059F9858 D7E2CFEE 300D0609

2A864886 F70D0101 05050003 8181001E 90C5FD47 56D31DCB BCBD13E4 2A0009FB

DC91A424 0AC71E52 7B29A280 6DAC8A24 6D393164 CA58596A 24C0656D A5CF1D06

7017D588 B96F2001 FDBD0708 5561AA9A 8EC32D85 D41FA7FE 8665CFAE 56622FB2

0AD3E942 04BCDD25 813A726F D2C3B0A1 3B595048 31319131 45830EE7 8F1AA0F9

CD087C2F D9AF468B 91E039C4 B3A3B7

quit

spanning-tree mode pvst

spanning-tree extend system-id

!

!

!

!

!

!

vlan internal allocation policy ascending

!

!

!

!

!

!

interface FastEthernet0

no ip address

!

interface GigabitEthernet1/0/1

switchport trunk allowed vlan 1,10,20,30

switchport mode trunk

!

interface GigabitEthernet1/0/2

switchport access vlan 20

switchport mode access

!

interface GigabitEthernet1/0/3

switchport access vlan 20

switchport mode access

!

interface GigabitEthernet1/0/4

switchport access vlan 20

switchport mode access

!

interface GigabitEthernet1/0/5

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/6

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/7

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/8

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/9

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/10

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/11

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/12

switchport access vlan 10

switchport mode access

!

interface GigabitEthernet1/0/13

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/14

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/15

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/16

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/17

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/18

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/19

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/20

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/21

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/22

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/23

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/24

switchport access vlan 30

switchport mode access

!

interface GigabitEthernet1/0/25

!

interface GigabitEthernet1/0/26

!

interface TenGigabitEthernet1/0/1

!

interface TenGigabitEthernet1/0/2

!

interface Vlan1

no ip address

!

ip http server

ip http secure-server

!

!

!

!

line con 0

line vty 0 4

login

line vty 5 15

login

!

end